How to use U-Boot on PHYTEC phyBOARD-i.MX6UL-Segin
--------------------------------------------------

- Configure and build U-Boot for phyCORE-i.MX6UL:

    $ make mrproper
    $ make phycore_pcl063_defconfig
    $ make

  This will generate SPL and u-boot-dtb.img images.

- The SPL and u-boot-dtb.img images need to be flashed into the micro SD card:

    $ sudo dd if=SPL of=/dev/mmcblk0 bs=1k seek=1; sync
    $ sudo dd if=u-boot-dtb.img of=/dev/mmcblk0 bs=1k seek=69; sync

- Jumper settings:

  JP1:   Open: Boot from NAND
       Closed: Boot from SD/MMC1

- Connect the Serial cable to UART0 and the PC for the console.

- Insert the micro SD card in the board and power it up.

- U-Boot messages should come up.
