* MediaTek Frame Engine Ethernet controller

Required properties:
- compatible: should be "mediatek,mt7628-eth"
- reg: address and length of the register set for the frame
       engine ethernet controller and the internal switch.
- syscon: phandle to the system controller

Example:

eth@10100000 {
	compatible = "mediatek,mt7628-eth";
	reg = <0x10100000 0x10000
	       0x10110000 0x8000>;

	syscon = <&sysc>;
};
