U-Boot for Freescale Vybrid VF610

This file contains information for the port of U-Boot to the Freescale Vybrid
VF610 SoC.

1. CONVENTIONS FOR FUSE ASSIGNMENTS
-----------------------------------

1.1 MAC Address: It is stored in fuse bank 4, with the 16 msbs in word 2 and the
    32 lsbs in word 3.
